MESH FILE_PATH cube.msh

E = 200e3
nu = 0.3

PHYSICAL_ENTITY left   BC u=0
PHYSICAL_ENTITY front  BC v=0
PHYSICAL_ENTITY bottom BC w=0

# PHYSICAL_ENTITY right  BC tx=-1
# PHYSICAL_ENTITY back   BC ty=2
# PHYSICAL_ENTITY top    BC tz=3
# 
# PHYSICAL_ENTITY right  BC ty=1 tz=1
# PHYSICAL_ENTITY back   BC tx=1 tz=1
# PHYSICAL_ENTITY top    BC tx=1 ty=1

PHYSICAL_ENTITY right  BC tx=-1 ty=1 tz=1
PHYSICAL_ENTITY back   BC ty=2  tx=1 tz=1
PHYSICAL_ENTITY top    BC tz=3  tx=1 ty=1


FINO_SOLVER PROGRESS_ASCII
FINO_STEP

MESH_POST FILE_PATH cube-out3.msh VECTOR u v w sigma sigma1 sigma2 sigma3

